# Snowdog Maintenance Log

2020-Dec-12

- Oil change with STP Engine Oil High Mileage 5W-30. One quart in engine brought to full, 85mL in gearbox.
- Spark plug change with NGK 6775. Old had a good deal of carbon buildup.
- Checked all wheels; spinning freely. No need to lube.
- Checked main belt tension; good.
- Tensioned chain and lubed with Amsoil MP HD. Was dry enough to squeak and a bit slack.
- Wiped down gas tank, motor, etc as it had a light coating of oil and/or spilled fuel residue.
- Applied a bit of grease to the slide bearings on the front CVT.
- Tightened up brake cable by adjusting nut at caliber end. Latching the brake wasn't locking up the drivetrain.